{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Hangnyomás szint","Fűtés","","Magas","dBA","","","48","48","50","50"]
["","Hűtés","","Magas","dBA","","","48","48","49","49"]
["Standard Accessories","Használati utasítás","","","","","","1","1","1","1"]
["","Telepítési utasítás","","","","","","1","1","1","1"]
["Hűtőközeg","GWP","","","","","","675","675","675","675"]
["","Feltöltés","","","kg","","","1.34","1.34","1.34","1.34"]
["","Type","","","","","","R-32","R-32","R-32","R-32"]
["Operation range","Hűtés","Környezeti","Max.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Fűtés","Környezeti","Max.","°C párás hőm.","","","18","18","18","18"]
["","","","Min.","°C párás hőm.","","","-20","-20","-20","-20"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","","","8","8","8","8"]
["Méretek","Berendezés","","Szélesség","mm","","","795","795","795","795"]
["","","","Mélység","mm","","","300","300","300","300"]
["","","","Magasság","mm","","","693","693","693","693"]
["Kompresszor","Type","","","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Súly","Berendezés","","","kg","","","50","50","50","50"]
["Power supply","Fázis","","","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","","","50","50","50","50"]
["","Feszültség","","","V","","","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","693","693"]
["","","","Szélesség","mm","795","795"]
["","","","Mélység","mm","300","300"]
["Tömeg","Egység","","","kg","50","50"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","43","43"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-20","-20"]
["","","","Max.","°C párás hőm.","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dBA","46","46"]
["","Fűtés","","Magas","dBA","46","46"]
["Hűtőközeg","Típus","","","","R-32","R-32"]
["","Töltet","","","kg","1.34","1.34"]
["","Töltet","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","10","10"]
["","Szintkülönbség","IU - OU","Max.","m","8","8"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]