{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Méretek","Egység","","Magasság","mm","870","870"]
["","","","Szélesség","mm","1,100","1,100"]
["","","","Mélység","mm","460","460"]
["Tömeg","Egység","","","kg","117","117"]
["Kompresszor","Típus","","","","Hermetikusan zárt csavarkompresszor","Hermetikusan zárt csavarkompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-20","-20"]
["","","","Max.","°C száraz hőm.","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-20","-20"]
["","","","Max.","°C párás hőm.","15","15"]
["Hangteljesítményszint","Hűtés","","","dB(A)","73","76"]
["","Fűtés","","","dB(A)","76 (1)","79 (1)"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","53","57"]
["","Fűtés","","Névl.","dB(A)","60","63"]
["Refrigerant","Típus","","","","R-32","R-32"]
["","Feltöltés","","","kg","5","5"]
["","GWP","","","","675","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","9.52"]
["","Gáz","","Külső átm.","mm","22.2","22.2"]
["","Csőhossz","Max.","OU - IU","m","100","100"]
["","","Rendszer","Terhelés nélkül","m","30","30"]
["","További hűtőközeg utántöltés","","","kg/m","Lásd az összeszerelési kézikönyvet","Lásd az összeszerelési kézikönyvet"]
["Standard Accessories","Telepítési utasítás","","","","1","1"]
["","Általános biztonsági óvintézkedések","","","","1","1"]
["","Szalagkötések","","","","2","2"]
["","F-gáz címke lehúzása","","","","1","1"]
["","Csatlakozó csövek","","","","6","6"]
["Power supply","fázis","","","","3~","3~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","380-415","380-415"]
["Áram - 50Hz","A biztosítékok maximálisan felvett áramerőssége (MFA)","","","A","20","20"]
["Notes","","","","","(1) - Az ENER Lot 21 szerint","(1) - Az ENER Lot 21 szerint"]