{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Méretek","Egység","","Magasság","pp","734","734","734"]
["","","","Szélesség","pp","870","870","870"]
["","","","Mélység","pp","373","373","373"]
["Tömeg","Egység","","","kg","52","52","52"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-20","-20","-20"]
["","","","Max.","°C száraz hőm.","52","52","52"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-21","-21","-21"]
["","","","Max.","°C párás hőm.","18","18","18"]
["Hangteljesítményszint","Hűtés","","","dB(A)","62","63","64"]
["","Fűtés","","","dB(A)","62","63","64"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","48","49","50"]
["","Fűtés","","Névl.","dB(A)","48","49","50"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","Töltet","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Töltet","","","tCO2Eq","1.05","1.05","1.05"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.52","12.7","12.7"]
["","Csőhossz","Max.","OU - IU","m","50","50","50"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)","0,02 (30m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","30","30","30"]
["Standard Accessories","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Standard Accessories","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]