{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Méretek","Berendezés","","Magasság","mm","1,680"]
["","","","Szélesség","mm","930"]
["","","","Mélység","mm","765"]
["Súly","Egység","","","kg","183.0"]
["Compressor","Type","","","","Hermetikusan zárt csavarkompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-5.0"]
["","","","Max.","°C száraz hőm.","46.0"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15.0"]
["","","","Max.","°C párás hőm.","15.0"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","78.0"]
["","Fűtés","","","dB(A)","78.0"]
["Hűtőközeg","Type","","","","R-410A"]
["","Feltöltés","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52"]
["","Gáz","","Külső átm.","mm","22.2"]
["","Csőhossz","Max.","OU - IU","m","100"]
["","","Rendszer","Terhelés nélkül","m","30"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Csatlakozó csövek","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","380-415"]
["Áram - 50Hz","A biztosítékok maximálisan felvett áramerőssége (MFA)","","","A","25"]
["Notes","","","","","(1) - Az FDQ beltéri egység külön áramellátással rendelkezik"]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon"]
["Méretek","Egység","","Magasság","mm","","1680"]
["","","","Szélesség","mm","","930"]
["","","","Mélység","mm","","765"]
["Tömeg","Egység","","","kg","","184.0"]
["Kompresszor","Típus","","","","","Hermetikusan zárt csavarkompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","-5.0"]
["","","","Max.","°C száraz hőm.","","46.0"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","-15.0"]
["","","","Max.","°C párás hőm.","","15.0"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","78.0"]
["","Fűtés","","","dB(A)","","78.0"]
["Hűtőközeg","Töltet","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Töltet","","","tCO2Eq","","19.4"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","12.70"]
["","Gáz","","Külső átm.","mm","","22.2"]
["","Csőhossz","Max.","OU - IU","m","","100"]
["","","Rendszer","Terhelés nélkül","m","","30"]
["Standard Accessories","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Áramellátás","Frekvencia","","","Hz","","50"]
["Áramerősség - 50Hz","A biztosítékok maximálisan felvett áramerőssége (MFA)","","","A","","25"]