{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","37.0","37.0","31.0","31.0"]
["","","","Közepes","dB(A)","34.0","34.0","28.0","28.0"]
["","","","Alacsony","dB(A)","29.0","29.0","25.0","25.0"]
["","Hűtés","","Közepes","dB(A)","32.0","32.0","28.0","28.0"]
["","","","Alacsony","dB(A)","29.0","29.0","25.0","25.0"]
["","","","Magas","dB(A)","35.0","35.0","30.0","30.0"]
["Standard Accessories","Használati utasítás","","","","1","1","1","1"]
["","Telepítési utasítás","","","","1","1","1","1"]
["","Leeresztő tömlő","","","","1","1","1","1"]
["","Az leeresztő tömlő fémbilincse","","","","1","1","1","1"]
["","Alátét a függesztőkerethez","","","","8","8","8","8"]
["","Csavarok","","","","40","40","40","40"]
["","Szigetelés a szereléshez","","","","2","2","2","2"]
["","Tömítések","","","","5","5","5","5"]
["","Bilincsek","","","","4","4","4","4"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","9.52"]
["","Gáz","","Külső átm.","mm","9.52","12.70","12.70","15.90"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Hűtés","","","dB(A)","60","60","56","56"]
["Méretek","Egység","","Szélesség","mm","700","700","1,000","1,000"]
["","","","Mélység","mm","800","800","800","800"]
["","","","Magasság","mm","245","245","245","245"]
["Burkolat","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["","Szín","","","","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)"]
["Tömeg","Egység","","","kg","28.0","28.0","35.0","35.0"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","150","150","150","150"]
["","","","Névl.","Pa","30","30","30","30"]
["","Légáramlási arány","Fűtés","Magas","m³/perc","15.0","15.0","18.0","18.0"]
["","","","Alacsony","m³/perc","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/perc","12.5","12.5","15.0","15.0"]
["","","Hűtés","Alacsony","m³/perc","10.5","10.5","12.5","12.5"]
["","","","Medium","m³/perc","12.5","12.5","15.0","15.0"]
["","","","Magas","m³/perc","15.0","15.0","18.0","18.0"]
["Leeresztési emelési magasság","mm","","","","625","625","625","625"]
["Power supply","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60","50/60"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon"]