{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B","FTXF20A2V1B (Archived)","FTXF20A5V1B (Archived)","FTXF25A2V1B (Archived)","FTXF25A5V1B (Archived)","FTXF35A2V1B (Archived)"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","40","","","","39","39","40","40","40"]
["","","","Közepes","dB(A)","35","","","","34","34","34","34","35"]
["","","","Csendes működés","dB(A)","21","","","","21","21","21","21","21"]
["","","","Alacsony","dB(A)","29","","","","28","28","28","28","29"]
["","Hűtés","","Medium","dB(A)","34","","","","33","33","33","33","34"]
["","","","Csendes működés","dB(A)","20","","","","20","20","20","20","20"]
["","","","Alacsony","dB(A)","27","","","","25","25","26","26","27"]
["","","","Magas","dB(A)","43","","","","39","39","40","40","43"]
["Standard Accessories","Telepítési utasítás","","","","1","","","","1","1","1","1","1"]
["","Használati utasítás","","","","1","","","","1","1","1","1","1"]
["","Infravörös távirányító","","","","1","","","","1","1","1","1","1"]
["","AAA szárazelemek","","","","2","","","","2","2","2","2","2"]
["","Távirányító tartó","","","","1","","","","1","1","1","1","1"]
["","Szerelőlemez","","","","1","","","","1","1","1","1","1"]
["","Beltéri egység rögzítő csavarja","","","","2","","","","2","2","2","2","2"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infravörös távszabályzó","","","","ARC470A1","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","","","","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.50","","","","9.50","9.50","9.50","9.50","9.50"]
["","Ürítés","","","","18","","","","18","18","18","18","18"]
["Áramfelvétel","Hűtés","","Névl.","kW","0.032","","","","0.017","0.017","0.019","0.019","0.032"]
["","Fűtés","","Névl.","kW","0.032","","","","0.020","0.020","0.020","0.020","0.032"]
["Sound power level","Hűtés","","","dB(A)","58","","","","55","55","55","55","58"]
["","Fűtés","","","dB(A)","58","","","","55","55","55","55","58"]
["Méretek","Egység","","Szélesség","mm","770","","","","770","770","770","770","770"]
["","","","Mélység","mm","225","","","","225","225","225","225","225"]
["","","","Magasság","mm","286","","","","286","286","286","286","286"]
["Burkolat","Szín","","","","Fehér","","","","Fehér","Fehér","Fehér","Fehér","Fehér"]
["Tömeg","Egység","","","kg","9.00","","","","9.00","9.00","9.00","9.00","9.00"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","11.5","","","","10.3","10.3","10.3","10.3","11.5"]
["","","","Alacsony","m³/perc","7.0","","","","6.5","6.5","6.7","6.7","7.0"]
["","","","Közepes","m³/perc","9.0","","","","8.4","8.4","8.6","8.6","9.0"]
["","","","Csendes működés","m³/perc","5.3","","","","5.3","5.3","5.3","5.3","5.3"]
["","","Hűtés","Alacsony","m³/perc","6.3","","","","5.9","5.9","6.1","6.1","6.3"]
["","","","Közepes","m³/perc","8.3","","","","7.9","7.9","8.1","8.1","8.3"]
["","","","Magas","m³/perc","11.5","","","","9.8","9.8","10.1","10.1","11.5"]
["","","","Csendes működés","m³/perc","4.5","","","","4.4","4.4","4.4","4.4","4.5"]
["Power supply","fázis","","","","1~","","","","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","","","","50","50","50","50","50"]
["","Feszültség","","","V","220-240","","","","220-240","220-240","220-240","220-240","220-240"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","0.029","0.032","0.032"]
["","Fűtés","","Névl.","kW","","0.032","0.035","0.035"]
["Burkolat","Szín","","","","","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","","295","295","295"]
["","","","Szélesség","mm","","990","990","990"]
["","","","Mélység","mm","","263","263","263"]
["Tömeg","Egység","","","kg","","13.5","13.5","13.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","16.8","17.3","17.3"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","14.4","14.8","14.8"]
["","","","Alacsony","m³/perc","","11.9","12.2","12.2"]
["","","","Csendes működés","m³/perc","","10.5","10.7","10.7"]
["","","Fűtés","Magas","m³/perc","","17.3","17.9","17.9"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","14.8","15.8","15.8"]
["","","Fűtés","Alacsony","m³/perc","","12.2","12.8","12.8"]
["","","","Csendes működés","m³/perc","","10.7","11.3","11.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","59","60","62"]
["","Fűtés","","","dB(A)","","61","62","62"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","43","45","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","39","41","42"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","34","36","37"]
["","","","Csendes működés","dB(A)","","31","33","34"]
["","Fűtés","","Magas","dB(A)","","42","44","45"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","38","40","41"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","33","35","36"]
["","","","Csendes működés","dB(A)","","30","32","33"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","","12.7","12.7","12.7"]
["","Ürítés","","","","","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Vezetékes távszabályzó","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2"]
["","Operation manual","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","2","2","2"]
["","Infrared remote control","","","","","1","1","1"]
["","Mounting plate","","","","","1","1","1"]
["","Remote control holder","","","","","1","1","1"]
["Áramellátás","Megnevezés","","","","","V1","V1","V1"]
["","fázis","","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","","50","50","50"]
["","Feszültség","","","V","","220-240","220-240","220-240"]