{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-N"]
[]
[]
[]
[]
["","","","","","RXTM30N2V1B","RXTM40N2V1B"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","49","49"]
["","Hűtés","","Névl.","dB(A)","48","48"]
["Standard Accessories","Telepítési utasítás","","","","1","1"]
["","Hűtőközeg töltési címke","","","","1","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","0.7","0.7"]
["","GWP","","","","675","675"]
["","Töltet","","","kg","1.1","1.1"]
["","Típus","","","","R-32","R-32"]
["Ventilátormotor","Sebesség","Hűtés","Szuper alacsony","1/perc","450","360"]
["","","Fűtés","Szuper alacsony","1/perc","360","360"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","15","15"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","763","763"]
["","","","Mélység","mm","312","312"]
["","","","Magasság","mm","551","551"]
["Tömeg","Egység","","","kg","38","38"]
["Power supply","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]
["Notes","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon"]