{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLCO2"]
[]
[]
[]
[]
["","","","","WLCO2."]
["A csatlakoztatható beltéri egységek maximális száma:","","","","0"]
["A csatlakoztatható kültéri egységek maximális száma: @","","","","0"]
["Burkolat","Szín","","","Fehér"]
["","Gomb burkolata","","","Nem"]
["","Üzemjelző LED","Szín","","Zöld"]
["Méretek","Egység","Magasság","mm","95"]
["","","Szélesség","mm","95.0"]
["","","Mélység","mm","62.0"]
["","Becsomagolt egység","Magasság","mm","565"]
["","","Szélesség","mm","375"]
["","","Mélység","mm","280"]
["Tömeg","Egység","","kg","0.126"]
["Csomagolás","Anyag","","","Kartonlemez"]
["","Súly","","kg","0.046"]
["Külső hőmérséklet","Működés","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Tárolás","Min.","°C","-20"]
["","","Max.","°C","60"]
["","Külső hőmérséklet-=-Relatív páratartalom <-=-%","","%","90"]
["Beszerelés","","","","Beltéri telepítés"]